!

! Last configuration change at 04:31:16 UTC Sun Aug 4 2024

!

version 15.5

service timestamps debug datetime msec

service timestamps log datetime msec

no service password-encryption

!

hostname ISP-LCL2

!

boot-start-marker

boot-end-marker

!

!

!

no aaa new-model

!

!

!

bsd-client server url https://cloudsso.cisco.com/as/token.oauth2

mmi polling-interval 60

no mmi auto-configure

no mmi pvc

mmi snmp-timeout 180

!

!

!

!

!

no ip icmp rate-limit unreachable

!

!

!

!

!

!

!

!

!

!

!

!

no ip domain lookup

no ip cef

no ipv6 cef

!

multilink bundle-name authenticated

!

!

!

!

!

!

!

cts logging verbose

!

!

!

redundancy

!

!

ip tcp synwait-time 5

!

!

!

!

!

!

!

!

!

!

!

!

!

interface Ethernet0/0

ip address 207.0.117.1 255.255.255.252

!

interface Ethernet0/1

ip address 205.0.115.2 255.255.255.252

!

interface Ethernet0/2

ip address 210.0.110.1 255.255.255.252

!

interface Ethernet0/3

no ip address

shutdown

!

interface Ethernet1/0

no ip address

shutdown

!

interface Ethernet1/1

no ip address

shutdown

!

interface Ethernet1/2

no ip address

shutdown

!

interface Ethernet1/3

no ip address

shutdown

!

interface Serial2/0

no ip address

shutdown

serial restart-delay 0

!

interface Serial2/1

no ip address

shutdown

serial restart-delay 0

!

interface Serial2/2

no ip address

shutdown

serial restart-delay 0

!

interface Serial2/3

no ip address

shutdown

serial restart-delay 0

!

interface Serial3/0

no ip address

shutdown

serial restart-delay 0

!

interface Serial3/1

no ip address

shutdown

serial restart-delay 0

!

interface Serial3/2

no ip address

shutdown

serial restart-delay 0

!

interface Serial3/3

no ip address

shutdown

serial restart-delay 0

!

router bgp 65001

bgp log-neighbor-changes

network 205.0.115.0 mask 255.255.255.252

network 207.0.117.0 mask 255.255.255.252

network 210.0.110.0 mask 255.255.255.252

neighbor 205.0.115.1 remote-as 65002

neighbor 207.0.117.2 remote-as 65001

neighbor 210.0.110.2 remote-as 65001

!

ip forward-protocol nd

!

!

no ip http server

no ip http secure-server

!

!

!

!

control-plane

!

!

!

!

!

!

!

!

line con 0

exec-timeout 0 0

privilege level 15

logging synchronous

line aux 0

exec-timeout 0 0

privilege level 15

logging synchronous

line vty 0 4

login

transport input none

!

!

end